Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	380	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	14/08/91	Elevation:	240 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7739295 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	487807  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granulite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Medium Non-	Principal Profile Form:	Dy2.33
	gravelly Sandy Clayey Shallow
	ASC Confidence:	Great Soil Group:	Solodized 
	No analytical data are available but confidence is fair.	solonetz
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Heteropogon contortus, 
	Bothriochloa pertusa	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.09 m	Dark greyish brown (10YR4/2-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy
	 fabric; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change 
	A2j	0.09 - 0.15 m	Yellowish brown (10YR5/4-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B21	0.15 - 0.45 m	Yellowish brown (10YR5/6-Moist); Mottles, 5YR58, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; 
	Coarse sandy medium clay; Strong grade of structure, 20-50 mm, Prismatic; Smooth-ped fabric; 
	Dry; Very strong consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.3); Clear change to - 
	C	0.45 - 0.8 m	; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	380	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	380	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile