Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	385	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	14/08/91	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7741687 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	490204  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Medium Non-gravelly Sandy 	Principal Profile Form:	Uc5.21
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - Aristida species
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Planchonia careya, Petalostigma pubescens
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus coolibah
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sand; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	, Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to - 
	A3	0.1 - 0.25 m	Brown (7.5YR4/3-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Diffuse change to - 
	B21	0.25 - 0.7 m	Yellowish red (5YR4/6-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.6); Clear change to - 
	2B2	0.7 - 0.9 m	Dark red (2.5YR3/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular blocky;
	 Smooth-ped fabric; Dry; Very firm consistence; 10-20%, medium gravelly, 6-20mm, angular, 
	Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	2B/C	0.9 - 1.1 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Sandstone, coarse fragments; , Calcareous, ,
	 ; , Gypseous, , ; Field pH 8 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	385	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	385	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile