Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	386	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	15/08/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7738693 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	399309  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Cracking, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Brown Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.34
	fine Very fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Cenchrus ciliaris, Dichanthium sericeum, Eragrostis 
	species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 0.51-1m, Sparse. *Species includes - Eucalyptus species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.07 m	Dark brown (10YR3/3-Moist); ; Silty medium clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	9.5 (Raupach, 0.05); Clear, Smooth change to - 
	A12	0.07 - 0.2 m	Brown (10YR4/3-Moist); ; Heavy clay; Strong grade of structure, 20-50 mm, Angular blocky; 
	Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Clear, Smooth 
	change to - 
	B1	0.2 - 0.45 m	Brown (7.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, 20-50 mm, Angular blocky; 
	Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), Manganiferous, Fine (0 -
	 2 mm), Nodules; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; 
	Field pH 9.5 (Raupach, 0.3); Gradual, Smooth change to - 
	B21	0.45 - 0.75 m	Brown (7.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), Manganiferous, 
	Medium (2 -6 mm), Nodules; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	386	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	8.4A
	0.2 - 0.45	9.3A
	0.45 - 0.75	8.9A	13.6J	9.4	0.1	0.7	21.1I	3.32
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07
	0.2 - 0.45
	0.45 - 0.75
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.2 - 0.45
	0.45 - 0.75

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	386	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension