Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	388	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	15/08/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7737698 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	403404  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Kandosol Medium Non-gravelly Silty 	Principal Profile Form:	Gn2.91
	Clay-loamy Shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Dichanthium sericeum
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 0.51-1m, Sparse. *Species includes - Eucalyptus species, Grevillea species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Apj	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); Mottles, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; Silty 
	light clay; Massive grade of structure; Earthy fabric; Dry; Strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 5.8 (Raupach, 0.05); Clear change to - 
	A12j	0.05 - 0.2 m	Brown (10YR5/3-Moist); Mottles, 10-20% , 0-5mm, Distinct; Mottles, 10-20% ; Sandy clay loam 
	(Heavy); Massive grade of structure; Earthy fabric; Dry; Strong consistence; 0-2%, fine 
	gravelly, 2-6mm, angular, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, 
	Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	B21c	0.2 - 0.38 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , 5-15mm, Distinct; Mottles, 20-50% ; Sandy
	 clay loam; Massive grade of structure; Earthy fabric; Dry; Strong consistence; 0-2%, fine 
	gravelly, 2-6mm, angular, Quartz, coarse fragments; Common (10 - 20 %), Ferromanganiferous,
	 Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	388	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	388	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile