Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	389	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	15/08/91	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7740300 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	401595  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	240 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Very thick Non-gravelly 	Principal Profile Form:	Dr2.23
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa ewartiana, Bothriochloa decipiens, 
	Heteropogon contortus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.04 m	Black (10YR2/1-Moist); ; Loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Clear, Smooth change to - 
	A12	0.04 - 0.25 m	Dark brown (7.5YR3/3-Moist); ; Coarse sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, Igneous rock (unidentified), 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Abrupt, 
	Smooth change to - 
	A21	0.25 - 0.45 m	Brown (7.5YR4/4-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.3); Gradual, Smooth 
	change to - 
	A22	0.45 - 0.65 m	Reddish yellow (7.5YR6/6-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry;
	 Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.6); Clear, Smooth 
	change to - 
	B21	0.65 - 0.7 m	Yellowish red (5YR4/6-Moist); ; Sandy light clay; Massive grade of structure; Earthy fabric; Dry;
	 Strong consistence; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	389	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	389	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile