Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	391	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	15/08/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7728705 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	406291  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mesonatric Brown Sodosol Thick Non-gravelly Silty 	Principal Profile Form:	Db1.33
	Clayey Very deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa ewartiana, Chrysopogon fallax
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.06 m	Dark brown (10YR3/3-Moist); ; Silty loam; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear, Smooth 
	change to - 
	A2j	0.06 - 0.3 m	Very dark greyish brown (10YR3/2-Moist); ; Silty loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to - 
	B21	0.3 - 0.6 m	Dark brown (10YR3/3-Moist); ; Silty light clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	7.5 (Raupach, 0.4); Gradual, Smooth change to - 
	2A1	0.6 - 1.2 m	Dark greyish brown (10YR4/2-Moist); Mottles, 7.5YR56, 0-2% , 0-5mm, Faint; Mottles, 0-2% ; 
	Sandy loam; Weak grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Strong consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Soft segregations; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.9); Abrupt, Smooth change to - 
	2A21e	1.2 - 1.42 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR56, 20-50% , 5-15mm, Prominent; Mottles, 
	7.5YR46, 20-50% ; Clayey sand; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Soft segregations; , Calcareous, 
	, ; , Gypseous, , ; 
	2A22e	1.42 - 1.7 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR56, 20-50% , 5-15mm, Prominent; Mottles, 
	7.5YR46, 20-50% ; Loamy sand; Weak grade of structure, 50-100 mm, Subangular blocky; 
	Smooth-ped fabric; Dry; Very strong consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 
	20 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 1.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	391	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.1A
	0.3 - 0.6	7.8A	6.5J	3.9	0.2	2.2	16.8I	13.10
	1.42 - 1.7	9.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.3 - 0.6
	1.42 - 1.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.3 - 0.6
	1.42 - 1.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	391	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension