Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	399	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	02/09/91	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7759199 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	398813  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	60 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Grey Chromosol Very thick Sandy	Principal Profile Form:	Dg4.42
	 Clayey Moderately deep 
	ASC Confidence:	Great Soil Group:	Soloth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eragrostis species, Heteropogon contortus
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus platyphylla, Melaleuca viridiflora
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus platyphylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR4/3-Moist); ; Coarse sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); 
	Diffuse change to - 
	A2e	0.08 - 0.6 m	Light brown (7.5YR6/4-Moist); ; Coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach,
	 0.3); Sharp change to - 
	B21	0.6 - 0.9 m	Light grey (10YR7/1-Moist); Mottles, 7.5YR58, 20-50% , 15-30mm, Prominent; Mottles, 20-50% ; 
	Coarse sandy medium clay; Strong grade of structure, 20-50 mm, Columnar; Smooth-ped fabric;
	 Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	399	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.9A
	0.08 - 0.6	6.1A
	0.6 - 0.9	6.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.6
	0.6 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.6
	0.6 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	399	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension