Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	40	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	17/07/90	Elevation:	342 metres
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7782914 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	385685  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Ferricrete 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	175 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Red Sodosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.22
	Clay-loamy Shallow
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida species, Chrysopogon fallax
	Mid Strata - Shrub, 1.01-3m, Isolated plants. *Species includes - Acacia species
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Acacia shirleyi, Eucalyptus papuana, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Sand; Massive grade of structure; Earthy fabric; Moderately 
	moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.04); 
	Few, fine (1-2mm) roots; Abrupt, Smooth change to - 
	A2	0.1 - 0.25 m	Brown (10YR4/3-Moist); ; Sand; Massive grade of structure; Earthy fabric; Moderately moist; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); Few, 
	fine (1-2mm) roots; Clear, Smooth change to - 
	B21c	0.25 - 0.45 m	Reddish brown (5YR5/4-Moist); ; Sandy clay loam (Heavy); Moderate grade of structure, 5-10 
	mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Very weak consistence; Common
	 (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ;
	 , Continuous; Field pH 6.5 (Raupach, 0.3); Few, fine (1-2mm) roots; Clear, Irregular change to - 
	C	0.45 - 0.7 m	Dark red (2.5YR3/6-Moist); Mottles, 2.5Y74, 10-20% , 0-5mm, Prominent; Mottles, 10-20% ; 
	Sandy clay loam; Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; 
	Ferricrete, Uncemented, Platy; Field pH 6 (Raupach, 0.5); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	40	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.8A	2.2B	0.69	0.16	0.03
	0.1 - 0.25	6.9A
	0.25 - 0.45	6.5A	1.3J	0.4	0.2	0.2	2.4I	8.33
	0.45 - 0.7	6.2A	1.4B	0.74	0.32	0.04
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.45
	0.45 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.45
	0.45 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	40	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension