Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	412	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	04/09/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7722096 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	431599  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Sandstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Yellow Kandosol Thin Non-gravelly Clay-	Principal Profile Form:	Gn2.32
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, <0.25m, Sparse. *Species includes - Eragrostis species, Aristida species
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus melanophloia
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	Clear change to - 
	A2j	0.05 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	B21	0.2 - 0.52 m	Brownish yellow (10YR6/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; Common (10 - 20 %), Manganiferous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); Clear change to - 
	B/C	0.52 - 0.9 m	; Massive grade of structure; Earthy fabric; Dry; Very firm consistence; 2-10%, medium 
	gravelly, 6-20mm, angular, dispersed, Sandstone, coarse fragments; Common (10 - 20 %), 
	Manganiferous, Coarse (6 - 20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	412	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	412	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile