Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	23/09/91	Elevation:	330 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7747056 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	417002  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Brown Chromosol Medium Non-	Principal Profile Form:	Dy3.42
	gravelly Loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Chrysopogon fallax, Heteropogon contortus, Aristida 
	species	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Grevillea parallela
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, rounded, Rhyolite
	Profile Morphology
	A1	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; Earthy
	 fabric; Dry; Weak consistence; 20-50%, medium gravelly, 6-20mm, rounded, Rhyolite, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A21	0.05 - 0.15 m	Dark yellowish brown (10YR4/5-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	A22e	0.15 - 0.2 m	Dark yellowish brown (10YR4/5-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B21	0.2 - 0.4 m	Yellowish brown (10YR5/4-Moist); Mottles, 2.5YR44, 20-50% , 0-5mm, Prominent; Mottles, 
	7.5YR56, 20-50% ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-
	ped fabric; Dry; Very firm consistence; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6
	 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	427	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile