Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	23/09/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7739300 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	415423  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mesonatric Red Sodosol Thick Non-gravelly Sandy 	Principal Profile Form:	Dr2.33
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodized 
	All necessary analytical data are available.	solonetz
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Chrysopogon fallax, Panicum species, Heteropogon 
	triticeus	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Eucalyptus brownii, Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Brown (7.5YR4/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; Dry; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear 
	change to - 
	A2	0.05 - 0.35 m	Yellowish red (5YR4/6-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear
	 change to - 
	A22j	0.35 - 0.4 m	Strong brown (7.5YR5/6-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B21	0.4 - 0.65 m	Reddish brown (5YR4/3-Moist); Mottles, 0-2% , 0-5mm, Faint; Mottles, 0-2% ; Fine sandy light 
	clay; Strong grade of structure, 20-50 mm, Columnar; Strong grade of structure, 2-5 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Veins; , Calcareous, , ; , Gypseous, , ; Gradual change to - 
	B22	0.65 - 1.1 m	Dark brown (7.5YR3/2-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6A	2.8B	1.4	0.34	0.09
	0.05 - 0.35	5.9A
	0.4 - 0.65	7.5A	5.2B	6.2	0.17	3.5	16.6I	21.08
	5.1J	6.3	0.2	2.6	15.66
	0.65 - 1.1	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.35
	0.4 - 0.65
	0.65 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.35
	0.4 - 0.65
	0.65 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension