Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	435	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	24/09/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7736054 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	410422  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Loamy 	Principal Profile Form:	Dr2.22
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	All necessary analytical data are available.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Dichanthium sericeum, Eragrostis species, 
	Cenchrus ciliaris	Mid Strata - Tree, 1.01-3m, Mid-dense. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 7 (Raupach, 0.05); Clear change to - 
	A3	0.08 - 0.27 m	Brown (7.5YR4/3-Moist); ; Fine sandy clay loam; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Clear change to - 
	B1	0.27 - 0.4 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Clear 
	change to - 
	B21	0.4 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Light clay; Strong grade of structure, 20-50 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; Very few (0 - 2 %), Manganiferous, 
	Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6);
	 Clear change to - 
	B22	0.6 - 1 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7
	 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	435	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.9A	4.2B	3.3	0.44	0.07
	0.4 - 0.6	6.3A	5.3B	6.2	0.23	0.23	13.6I	1.69
	5.5J	5.8	0.3	0.4	2.94
	0.6 - 1	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.4 - 0.6
	0.6 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.4 - 0.6
	0.6 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	435	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension