Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	437	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	14/10/91	Elevation:	271 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7707125 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	424548  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Chromosol Thick Non-gravelly 	Principal Profile Form:	Db2.32
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Chrysopogon fallax, 
	Aristida species	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus species, Melaleuca species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus papuana, Eucalyptus coolibah, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; 
	Earthy fabric; Dry; Common (10 - 20 %), , , ; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.05); 
	A2j	0.12 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Common (10 - 20 %), , , ; , Calcareous, , ; , Gypseous, , ; 
	A3	0.2 - 0.35 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Few (2 - 
	10 %), , , ; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); 
	B21	0.35 - 0.65 m	Dark yellowish brown (10YR4/4-Moist); Mottles, 7.5YR46, 2-10% , 0-5mm, Distinct; Mottles, 2-
	10% ; Sandy light clay; Weak grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; 
	Dry; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.6); 
	B22	0.65 - 1.1 m	; Coarse sand; Massive grade of structure; Sandy (grains prominent) fabric; Dry; , Calcareous, 
	, ; , Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	437	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.1A
	0.35 - 0.65	6.2A	3.4J	1.6	0.3	0.2	6.1I	3.28
	0.65 - 1.1	6.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.35 - 0.65
	0.65 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.35 - 0.65
	0.65 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	437	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension