Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	439	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	14/10/91	Elevation:	243 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7704853 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	419062  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Crusty Brown Vertosol Gravelly Very fine 	Principal Profile Form:	Ug6.5
	Very fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Closed or dense. *Species includes - Eulalia aurea, Bothriochloa species, 
	Sporobolus species	Mid Strata - Shrub, 1.01-3m, Isolated plants. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, rounded, Quartz
	Profile Morphology
	A1j	0 - 0.03 m	Dark grey (10YR4/1-Moist); ; Medium clay; Massive grade of structure; Dry; Strong 
	consistence; , Calcareous, , ; , Gypseous, , ; 
	A2	0.03 - 0.2 m	Dark grey (10YR4/1-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moderate grade of structure, 5-10 mm, Angular blocky; Dry; Strong consistence; Very 
	few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.05); 
	B21	0.2 - 0.4 m	Grey (10YR5/1-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, Angular blocky; 
	Moderate grade of structure, 2-5 mm; Moderately moist; Very firm consistence; Very few (0 - 2 
	%), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; Field pH 9.5 (Raupach, 0.3); 
	B22	0.4 - 0.9 m	Brown (10YR5/3-Moist); ; Light medium clay; Massive grade of structure; Moderately moist; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	439	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.2	6.6A
	0.2 - 0.4	6.6A	8J	10.6	0.1	2.2	26.8I	8.21
	0.4 - 0.9	7.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.2
	0.2 - 0.4
	0.4 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.2
	0.2 - 0.4
	0.4 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	439	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension