Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	452	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	17/10/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7683428 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	432224  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	10 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Endohypersodic Black Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.16
	fine Very fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Sporobolus species, Cyperus species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Acacia argyrodendron
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, Angular 
	blocky; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	Clear change to - 
	B21	0.1 - 0.3 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay; Moderate grade of structure, 10-20 
	mm, Angular blocky; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is 
	Moderately calcareous; Gradual change to - 
	B22	0.3 - 0.6 m	Very dark grey (10YR3/1-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is Moderately 
	calcareous; Field pH 9.5 (Raupach, 0.4); Gradual change to - 
	B23	0.6 - 0.9 m	Dark grey (10YR4/1-Moist); ; Light clay; Weak grade of structure, 50-100 mm, Prismatic; Dry; 
	Very firm consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is Moderately calcareous; 
	Field pH 9.5 (Raupach, 0.8); Gradual change to - 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	452	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.3A
	0.1 - 0.3	13.1J	5.8	0.1	2	23.5I	8.51
	0.3 - 0.6	8.2A
	0.6 - 0.9	7.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.6
	0.6 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	452	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension