Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	462	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	04/11/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7718590 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	432020  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Crusty Grey Vertosol Non-gravelly Medium fine Medium	Principal Profile Form:	Ug5
	 fine Moderately deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Elytrophorus spicatus, Nicotiana species, Panicum 
	species	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Shrub, 1.01-3m, Sparse. *Species includes - Atalaya hemiglauca, Lysiphillum carronii, Bursaria incana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.05); Gradual change to - 
	A12	0.05 - 0.35 m	Dark grey (10YR4/1-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.3); Gradual change to - 
	B2	0.35 - 0.8 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Weak grade of structure, 50-100 mm, Angular 
	blocky; Smooth-ped fabric; Moderately moist; Strong consistence; , Calcareous, , ; , Gypseous, 
	, ; Field pH 6.5 (Raupach, 0.6); Gradual change to - 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	462	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	462	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile