Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	48	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	19/07/90	Elevation:	480 metres
	Map Ref.:	Sheet No. : 7956   GPS	Rainfall:	No Data
	Northing/Long.:	7721854 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	327320  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	160 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol Thin Non-gravelly Sandy 	Principal Profile Form:	Gn2.12
	Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Chrysopogon fallax, Themeda triandra, 
	Enneapogon species	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Bursaria incana, Grevillea glauca
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus similis, Eucalyptus erythrophloia, Eucalyptus setosa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Reddish brown (5YR4/4-Moist); ; Sand; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.5 (Raupach, 0.04); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B1	0.08 - 0.4 m	Red (2.5YR4/6-Moist); ; Loamy sand (Light); Weak grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Common, fine (1-2mm) roots; Gradual, Smooth 
	change to - 
	B21	0.4 - 1.05 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.3 (Raupach, 0.6); Few, fine (1-2mm) roots; Gradual, Smooth change to - 
	B22	1.05 - 2.05 m	Red (2.5YR4/6-Moist); ; Sandy clay loam (Light); Weak grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; , Calcareous, , ; , Gypseous, ,
	 ; Field pH 6 (Raupach, 1.2); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	48	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.1A	2.2B	0.38	0.13	0.03
	0.08 - 0.4	6.7A
	0.4 - 1.05	6.6A	1.6J	1	0.2	0	2.2I	0.00
	1.05 - 2.05	6.6A	0.99B	1.3	0.04	0.04
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.4
	0.4 - 1.05
	1.05 - 2.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.4
	0.4 - 1.05
	1.05 - 2.05

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	48	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension