Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	496	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	20/11/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7683685 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	465286  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Self-Mulching Black Vertosol Non-gravelly 	Principal Profile Form:	Ug5.13
	Very fine Very fine Deep 
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Cenchrus ciliaris
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, subrounded, Diorite
	Profile Morphology
	A1	0 - 0.08 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; Strong grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Moist; Firm consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm),
	 Nodules; , Gypseous, , ; 
	B2	0.08 - 1.1 m	Black (10YR2/1-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Lenticular; Smooth-
	ped fabric; Dry; Rigid consistence; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; 
	B/C	1.1 - 1.4 m	Light olive brown (2.5Y5/4-Moist); Mottles, 10YR54, 10-20% , 0-5mm, Faint; Mottles, 10-20% ; 
	Heavy clay; Moderate grade of structure, 10-20 mm, Lenticular; Smooth-ped fabric; Dry; Very 
	strong consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; Many (20 -
	 50 %), Calcareous, Coarse (6 - 20 mm), Nodules; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	496	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8A
	0.08 - 1.1	8.2A	33J	15	0.2	1.7	48.2I	3.53
	1.1 - 1.8	8.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 1.1
	1.1 - 1.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 1.1
	1.1 - 1.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	496	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension