Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	510	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	09/04/90	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7820803 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	437644  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Limestone 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	160 degrees
	Surface Soil Condition (dry):	Cracking, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol Medium Non-gravelly 	Principal Profile Form:	Ug5.37
	Clayey Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Bothriochloa pertusa, 
	Bothriochloa ewartiana	Mid Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.12 m	Very dark grey (7.5YR3/1-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Field pH 7 (Raupach, 
	0.05); Sharp, Smooth change to - 
	B2	0.12 - 0.3 m	Reddish brown (2.5YR4/4-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; 20-50%, cobbly, 
	60-200mm, angular platy, stratified, Metamorphic rock (unidentified), coarse fragments; Many 
	(20 - 50 %), Calcareous, Medium (2 -6 mm), Concretions; , Gypseous, , ; Soil matrix is Highly 
	calcareous; Field pH 7.5 (Raupach, 0.3); Sharp, Smooth change to - 
	BC	0.3 - 0.6 m	Reddish brown (2.5YR5/4-Moist); ; Light medium clay; Moderate grade of structure, Subangular 
	blocky; Moderately moist; Firm consistence; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), 
	Concretions; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 (Raupach, 0.6); Sharp,
	 Irregular change to - 
	C	0.6 - 0.65 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	510	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	7.6A
	0.12 - 0.3	8.3A	27.2J	1.1	0.6	0.3	23.4I	1.28
	0.3 - 0.6	8.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	510	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension