Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	516	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	10/04/91	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7799608 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	433909  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Level
	Slope:	1 % 	Aspect:	190 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Red Chromosol Medium Non-gravelly Loamy 	Principal Profile Form:	Dr2.22
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	Analytical data are incomplete but reasonable confidence.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Phynchelytrum repens, Heteropogon contortus, 
	Themeda triandra	Mid Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana, Eucalyptus 
	crebra
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus 
	erythrophloia
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (7.5YR3/4-Moist); ; Coarse sandy loam (Light); Weak grade of structure, 10-20 mm,
	 Subangular blocky; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Few, very 
	fine (0-1mm) roots; Clear, Smooth change to - 
	A2	0.08 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam (Light); Weak grade of structure, 10-20 mm, 
	Subangular blocky; , Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) roots; Clear, 
	Smooth change to - 
	B1	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Sandy light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); Clear, Smooth 
	change to - 
	B2	0.3 - 0.85 m	Yellowish red (5YR5/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular
	 blocky; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Diffuse, Smooth change to - 
	BC	0.85 - 1 m	Yellowish red (5YR5/8-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); Clear, Wavy 
	change to - 
	C	1 - 1.2 m	; Massive grade of structure; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.15); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	516	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.6A
	0.2 - 0.3	6.5A	5.6J	2.7	0.8	0.4	8.4I	4.76
	0.3 - 0.85	6.7A
	0.85 - 1	6.5A
	1 - 1.2	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.2 - 0.3
	0.3 - 0.85
	0.85 - 1
	1 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.2 - 0.3
	0.3 - 0.85
	0.85 - 1
	1 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	516	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension