Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	518	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	11/04/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7771109 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	485338  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granite 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	100 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol Slightly gravelly Sandy 	Principal Profile Form:	Uc1.22
	Shallow  
	ASC Confidence:	Great Soil Group:	Lithosol
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa pertusa, Heteropogon contortus, 
	Eragrostis species	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus crebra, Planchonia careya
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.05); Few, fine (1-
	2mm) roots; Clear, Smooth change to - 
	A12	0.05 - 0.25 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 50-90%, medium gravelly, 6-20mm, subangular, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) 
	roots; Clear, Smooth change to - 
	C	0.25 - 0.4 m	Brownish yellow (10YR6/6-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 50-90%, medium gravelly, 6-20mm, subangular, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.4); , very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	518	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A
	0.25 - 0.4	6.8A	1.9J	1.2	0.3	0.5	3.6I	13.89
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.25 - 0.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.25 - 0.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	518	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension