Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	11/04/91	Elevation:	240 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7766739 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	487003  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Diorite 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	30 degrees
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Lithocalcic Red Dermosol Thin Non-gravelly Clayey 	Principal Profile Form:	Uf
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	Highly disturbed, for example, quarrying, roadworks, mining, landfill, urban
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa pertusa
	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay; Smooth-ped fabric; Moderately moist;
	 Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Few, very 
	fine (0-1mm) roots; 
	B	0.05 - 0.28 m	Dark brown (7.5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 2-5 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; 0-2%, medium gravelly,
	 6-20mm, subangular, dispersed, Substrate material, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Few, very fine (0-1mm) roots; 
	BC	0.28 - 0.4 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Massive grade of structure; Earthy 
	fabric; Moderately moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, 
	Substrate material, coarse fragments; Many (20 - 50 %), Calcareous, Medium (2 -6 mm), Soft 
	segregations; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8 (Raupach, 0.3); 
	Ck	0.4 - 1.1 m	; Massive grade of structure; Earthy fabric; Moderately moist; Very weak consistence; Very 
	many (50 - 100 %), Calcareous, Medium (2 -6 mm), Soft segregations; , Gypseous, , ; Soil 
	matrix is Highly calcareous; Field pH 9.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.9A
	0.28 - 0.4	7.2A	25.3J	4.2	0.1	0.4	26.2I	1.53
	0.4 - 1.1	8.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.28 - 0.4
	0.4 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.28 - 0.4
	0.4 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension