Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	11/04/91	Elevation:	220 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7751192 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	488110  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granite 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	30 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Paralithic Orthic Tenosol Thin Non-gravelly Sandy 	Principal Profile Form:	Uc4.21
	Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Sparse. *Species includes - Heteropogon contortus, Aristida species
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Planchonia careya, Eucalyptus species, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus papuana, Eucalyptus 
	platyphylla
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.08 m	Dark yellowish brown (10YR3/4-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, subangular, 
	dispersed, Granite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.05); Many, very fine (0-1mm) roots; Clear change to - 
	A2	0.08 - 0.3 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 10-20%, fine gravelly, 2-6mm, subangular, 
	dispersed, Granite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.3); Common, very fine (0-1mm) roots; Clear change to - 
	B	0.3 - 0.6 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Granite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 
	0.6); Few, very fine (0-1mm) roots; Gradual change to - 
	BC	0.6 - 0.9 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Granite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 
	0.9); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.3A
	0.08 - 0.3	7.5A	3.4J	0.8	0.3	0.4	2I	20.00
	0.3 - 0.6	7.6A
	0.6 - 0.9	7.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.6
	0.6 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	524	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension