Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	536	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	19/06/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7783607 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	423396  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	280 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol Thin Non-gravelly Clay-	Principal Profile Form:	Db1.13
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Phynchelytrum repens
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Reddish brown (5YR4/4-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9 
	(Raupach, 0.05); 
	B21	0.05 - 0.4 m	Brown (7.5YR4/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular
	 blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Common (10 - 20 %), 
	Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; Soil matrix is Highly calcareous; Field 
	pH 9 (Raupach, 0.3); 
	B22	0.4 - 0.7 m	Brown (10YR4/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky;
	 Smooth-ped fabric; Moderately moist; Very firm consistence; Common (10 - 20 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; Many (20 - 50 %), Calcareous, Medium (2 -6 mm), 
	Nodules; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9 (Raupach, 0.6); 
	B23k	0.7 - 0.85 m	Strong brown (7.5YR4/6-Moist); Mottles, 10YR34, 2-10% , 5-15mm, Distinct; Mottles, 2-10% ; 
	Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Strong consistence; Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Many (20 - 50 %), Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; Soil matrix 
	is Highly calcareous; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	536	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.8A
	0.05 - 0.4	7.8A	14J	3.2	0.2	0.5	16.6I	3.01
	0.4 - 0.7	8.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.4
	0.4 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.4
	0.4 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	536	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension