Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	547	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	20/06/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7797591 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	404410  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	150 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Um5.51
	loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Bothriochloa ewartiana, Phynchelytrum repens, 
	Heteropogon contortus	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus species
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus 
	erythrophloia
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR3/3-Moist); ; Sandy clay loam (Light); Massive grade of structure; 
	Very few (0 - 2 %), Ferromanganiferous, , ; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	A12	0.05 - 0.25 m	Dark reddish brown (2.5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Very few
	 (0 - 2 %), Ferromanganiferous, , ; , Calcareous, , ; , Gypseous, , ; 
	A3	0.25 - 0.6 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Very few (0 - 2 %), 
	Ferromanganiferous, , ; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Field pH 7 
	(Raupach, 0.6); 
	B2	0.6 - 1 m	Red (2.5YR4/8-Moist); , 7.5YR68; Clay loam, sandy; Massive grade of structure; Very few (0 - 
	2 %), Ferromanganiferous, , ; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 1); 
	B3c	1 - 1.1 m	; Massive grade of structure; Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	547	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A
	0.25 - 0.6	5.7A
	0.6 - 1	6.1A
	1 - 1.1	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.25 - 0.6
	0.6 - 1
	1 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.25 - 0.6
	0.6 - 1
	1 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	547	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension