Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	549	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	20/06/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7800254 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	418905  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Terrace (alluvial)
	3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Terrace plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Yellow Chromosol Thick Non-gravelly Loamy 	Principal Profile Form:	Dy2.23
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Closed or dense. *Species includes - Heteropogon contortus, Bothriochloa 
	ewartiana, Bothriochloa decipiens	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus brownii, Eucalyptus crebra, Eucalyptus 
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Dark yellowish brown (10YR3/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 
	A12	0.05 - 0.15 m	Dark brown (7.5YR3/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; 
	A2	0.15 - 0.45 m	Strong brown (7.5YR4/6-Moist); ; Clayey fine sand; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	B21	0.45 - 1.1 m	Dark yellowish brown (10YR4/6-Moist); ; Fine sandy light clay; Moderate grade of structure, 10-
	20 mm, Subangular blocky; Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped 
	fabric; Moderately moist; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.9); 
	B22k	1.1 - 1.4 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; Common (10 - 20 %), Calcareous, Medium (2 -6 
	mm), Soft segregations; , Gypseous, , ; Field pH 9.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	549	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A
	0.15 - 0.45	7.2A
	0.45 - 1.1	7.1A
	1.1 - 1.4	8.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.15 - 0.45
	0.45 - 1.1
	1.1 - 1.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.15 - 0.45
	0.45 - 1.1
	1.1 - 1.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	549	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension