Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	584	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	22/05/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158-1   GPS	Rainfall:	No Data
	Northing/Long.:	7827002 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	426677  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Siltstone 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	60 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Calcic Red Chromosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.32
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Heteropogon contortus, Bothriochloa species, Chrysopogon fallax
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.15 m	Reddish brown (5YR4/4-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; Slightly plastic; Normal plasticity; Non-sticky; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.05); Few, fine (1-2mm) roots; Sharp change to - 
	B21	0.15 - 0.35 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, Prismatic; 
	Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately moist; 
	Very firm consistence; Moderately plastic; Normal plasticity; Slightly sticky; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.7 (Raupach, 0.3); Few, fine (1-2mm) roots; Clear change to - 
	B22	0.35 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Strong grade of structure, 20-50 mm, Angular blocky; Strong 
	grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Strong 
	consistence; Very plastic; Normal plasticity; Slightly sticky; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7.5 (Raupach, 0.5); Few, fine (1-2mm) roots; Clear change to - 
	C	0.5 - 0.6 m	; Moderately moist; 50-90%, medium gravelly, 6-20mm, angular platy, dispersed, Siltstone, 
	coarse fragments; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Soft segregations; , 
	Gypseous, , ; Soil matrix is Moderately calcareous; Field pH 8.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	584	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.3A
	0.15 - 0.35	6.5A
	0.35 - 0.5	6.9A
	0.5 - 0.6	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.35
	0.35 - 0.5
	0.5 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.35
	0.35 - 0.5
	0.5 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	584	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension