Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	59	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	24/07/90	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7802736 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	410423  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	Dr2.12
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	Analytical data are incomplete but reasonable confidence.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Bothriochloa ewartiana, Bothriochloa pertusa
	Mid Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Planchonia careya
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, subrounded, Basalt
	Profile Morphology
	A1	0 - 0.12 m	Dark reddish brown (5YR3/2-Moist); ; Sandy clay loam; Strong grade of structure, 10-20 mm, 
	Polyhedral; Strong grade of structure, <2 mm, Granular; Smooth-ped fabric; Moderately moist; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Common, 
	very fine (0-1mm) roots; Clear, Smooth change to - 
	A3	0.12 - 0.28 m	Dark reddish brown (5YR3/3-Moist); ; Sandy light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Very weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B21	0.28 - 0.8 m	Red (2.5YR4/8-Moist); Mottles, 10YR46, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ; Sandy 
	light clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-ped fabric; Moist;
	 Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.3 (Raupach, 0.3); Field pH 7
	 (Raupach, 0.6); Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B22c	0.8 - 1 m	Strong brown (7.5YR5/8-Moist); ; Moist; Many (20 - 50 %), Ferromanganiferous, Very coarse 
	(20 - 60 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	59	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.5A	6.4B	1.9	0.74	0.09
	0.28 - 0.8	6.7A	5.5J	2	0.3	0.1	8.1I	1.23
	0.8 - 1	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.28 - 0.8
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.28 - 0.8
	0.8 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	59	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension