Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	597	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	22/05/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158-4   GPS	Rainfall:	No Data
	Northing/Long.:	7826016 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	418756  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Summit surface	Slope Category:	Gently inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Mottled-Subnatric Yellow Sodosol Thick Non-	Principal Profile Form:	Dy3.43
	gravelly Sandy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Heteropogon contortus, Panicum species, Heteropogon triticeus
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Fine sand; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	A12	0.05 - 0.15 m	Dark brown (10YR3/3-Moist); ; Fine sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; 
	A2e	0.15 - 0.45 m	Brown (10YR4/3-Moist); ; Fine sand (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Abrupt change 
	to - 
	B21	0.45 - 0.7 m	Brown (10YR5/3-Moist); Substrate influence, 10YR68, 20-50% , 5-15mm, Distinct; Substrate 
	influence, 2.5YR46, 20-50% ; Medium clay; Moderate grade of structure, 20-50 mm, Subangular
	 blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.8 (Raupach, 0.6); 
	B22c	0.7 - 1.2 m	Brown (10YR5/3-Moist); Substrate influence, 10YR68, 10-20% , 5-15mm, Distinct; Substrate 
	influence, 2.5YR46, 10-20% ; Medium clay; Moderate grade of structure, 50-100 mm, Prismatic; 
	Weak grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; 
	Strong consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; 
	B23k	1.2 - 1.65 m	Brown (10YR5/3-Moist); Substrate influence, 10YR68, 10-20% , 5-15mm, Distinct; Substrate 
	influence, 2.5YR46, 10-20% ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular
	 blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common (10 - 20 %), 
	Calcareous, Medium (2 -6 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 1.5); 
	B24	1.65 - 2.1 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Very few (0 - 
	2 %), Calcareous, Medium (2 -6 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	597	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	597	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.4A
	0.05 - 0.15	6.5A
	0.15 - 0.45	7.2A
	0.45 - 0.7	8.6A
	0.7 - 1.2	8.9A
	1.2 - 1.65	9.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.15
	0.15 - 0.45
	0.45 - 0.7
	0.7 - 1.2
	1.2 - 1.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.15
	0.15 - 0.45
	0.45 - 0.7
	0.7 - 1.2
	1.2 - 1.65

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	597	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension