Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	6	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	20/06/90	Elevation:	310 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7780662 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	477635  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol Medium Slightly gravelly 	Principal Profile Form:	Dr2.12
	Loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	Analytical data are incomplete but reasonable confidence.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa pertusa, Heteropogon contortus
	Mid Strata - , , . *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sandy loam; Moderate grade of structure, 
	2-5 mm, Granular; Earthy fabric; Moist; Very weak consistence; 2-10%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.05); Common, medium (2-5mm) roots; Gradual, Smooth change to - 
	B21t	0.15 - 0.55 m	Yellowish red (5YR4/6-Moist); ; Light clay; Strong grade of structure, 20-50 mm, Prismatic; 
	Strong grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Moist; Very firm 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; Few 
	cutans, <10% of ped faces or walls coated, faint; , Calcareous, , ; , Gypseous, , ; Field pH 6.2 
	(Raupach, 0.3); Common, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B3	0.55 - 0.72 m	Strong brown (7.5YR5/8-Moist); Substrate influence, 5YR54, 20-50% , 5-15mm, Distinct; 
	Substrate influence, 10YR31, 20-50% ; Clay loam; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Moist; Very firm consistence; 2-10%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2
	 -6 mm), Concretions; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Few, very fine 
	(0-1mm) roots; Clear, Smooth change to - 
	C	0.72 - 0.9 m	; Weak grade of structure, 5-10 mm, Polyhedral; Moist; Firm consistence; 10-20%, fine gravelly, 
	2-6mm, angular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, 
	Medium (2 -6 mm), Concretions; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	6	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.1A	5.1B	1.3	0.46	0.04
	0.15 - 0.55	8.1A	8.8B	3.3	0.21	0.19	17.2I	1.10
	10.2J	3.2	0.2	0	0.00
	0.72 - 0.9	8.4A	8.9B	3.2	0.1	0.22
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.55
	0.72 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.55
	0.72 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	6	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension