Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	62	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	24/07/90	Elevation:	285 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7804381 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	403441  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thin Slightly gravelly Clayey 	Principal Profile Form:	Uf6.31
	Clayey Very shallow
	ASC Confidence:	Great Soil Group:	Euchrozem
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa decipiens, Bothriochloa pertusa
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Eucalyptus 
	papuana
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, subangular, Basalt
	Profile Morphology
	A1	0 - 0.03 m	Dark red (2.5YR3/5-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-
	ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , Gypseous, , ; Many, fine (1-
	2mm) roots; Clear, Smooth change to - 
	B21	0.03 - 0.15 m	Dark red (2.5YR3/5-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-
	ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.2 
	(Raupach, 0.1); Many, fine (1-2mm) roots; Abrupt, Smooth change to - 
	C	0.15 - 0.3 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	62	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.15	6.7A	9.7B	4.1	1.4	0.08	14.4I	0.56
	9.4J	4.5	1.1	0.2	1.39
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.15
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.15

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	62	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension