Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	63	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	24/07/90	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7806375 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	401681  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.12
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Chloris species, Bothriochloa pertusa, Chrysopogon 
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Eucalyptus melanophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus erythrophloia, 
	Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.12 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.8 (Raupach, 0.05); Common, fine (1-2mm) roots; Clear, Smooth change 
	B21	0.12 - 0.6 m	Red (2.5YR4/6-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Weak consistence; Common cutans, 10-50% of ped 
	faces or walls coated, faint; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); Field pH 7 (Raupach, 0.6); 
	Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B22	0.6 - 1 m	Red (2.5YR4/6-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Firm consistence; Common cutans, 10-50% of ped faces 
	or walls coated, faint; , Calcareous, , ; , Gypseous, , ; Few, fine (1-2mm) roots; Abrupt, Smooth 
	change to - 
	B/C	1 - 1.15 m	Red (2.5YR4/6-Moist); Substrate influence, 7.5YR58, 20-50% , 5-15mm, Prominent; Substrate 
	influence, 10YR21, 20-50% ; Strong grade of structure, 10-20 mm, Subangular blocky; Smooth-
	ped fabric; Moderately moist; Weak consistence; Many (20 - 50 %), Manganiferous, Coarse (6 -
	 20 mm), Veins; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to - 
	C	1.15 - 1.2 m	; , Calcareous, , ; , Gypseous, , ; Field pH 7.2 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	63	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.9A	9.3B	3.9	2.4	0.1
	0.12 - 0.6	6.8A	7.7J	3.9	0.6	0	12.1I	0.00
	0.6 - 1	6.8A	5.8B	3.7	0.35	0.15
	1.15 - 1.2	7.5A	11B	7.1	0.09	0.33
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.6
	0.6 - 1
	1.15 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.6
	0.6 - 1
	1.15 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	63	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension