Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	676	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	18/07/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8255   GPS	Rainfall:	No Data
	Northing/Long.:	7650910 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	483917  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Dolerite 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Black Vertosol 	Principal Profile Form:	Ug5.13
	Slightly gravelly Medium fine Very fine Deep 
	ASC Confidence:	Great Soil Group:	Black earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Echinochloa colona
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Terminalia oblongata, Acacia harpophylla
	Surface Coarse Fragments:	2-10%, stony, 200-600mm, rounded, Dolerite
	Profile Morphology
	A1	0 - 0.25 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, 100-200 mm, 
	Subangular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.05); 
	B2	0.25 - 1.1 m	Very dark greyish brown (10YR3/2-Moist); ; Heavy clay; Strong grade of structure, 100-200 
	mm, Lenticular; Strong grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; Many cutans, >50% of ped faces or walls coated, 
	prominent; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; Soil 
	matrix is Moderately calcareous; Field pH 9.5 (Raupach, 0.6); 
	B22	1.1 - 1.4 m	Brown (10YR4/3-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Many cutans, >50% of ped faces 
	or walls coated, prominent; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Soft 
	segregations; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; 
	Soil matrix is Moderately calcareous; Field pH 9 (Raupach, 1.2); Field pH 9 (Raupach, 1.4); 
	C	1.4 - 1.45 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	676	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.25	8.6A
	0.25 - 1.1	8.7A	20.2J	24	0.1	6.7	48.2I	13.90
	1.1 - 1.4	8.3A
	1.4 - 	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.25
	0.25 - 1.1
	1.1 - 1.4
	1.4 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.25
	0.25 - 1.1
	1.1 - 1.4
	1.4 - 

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	676	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension