Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	685	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	30/07/91	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8258   GPS	Rainfall:	No Data
	Northing/Long.:	7808942 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	448620  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	60 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Grey Sodosol Thick Non-gravelly 	Principal Profile Form:	Dy5.82
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Soloth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Eragrostis species
	Mid Strata - Tree, 1.01-3m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus brownii, Planchonia careya
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (10YR3/3-Moist); ; Coarse sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear 
	change to - 
	A12	0.08 - 0.12 m	Brown (10YR4/3-Moist); ; Coarse sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	A21e	0.12 - 0.45 m	Yellowish brown (10YR5/4-Moist); ; Coarse sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; Loose consistence; 0-2%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.3); Abrupt change to - 
	A22	0.45 - 0.48 m	Very pale brown (10YR7/4-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; 
	Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Duripan, Moderately cemented, Continuous, 
	Massive; Abrupt change to - 
	B21	0.48 - 0.55 m	Light yellowish brown (2.5Y6/4-Moist); Mottles, 10YR56, 2-10% , 5-15mm, Distinct; Mottles, 2-
	10% ; Coarse sandy light clay; Massive grade of structure; Earthy fabric; Moderately moist; 
	Very strong consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Gradual change to - 
	C	0.55 - 0.7 m	; Very strong consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	685	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.8A
	0.55 - 0.7	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.55 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.55 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	685	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension