Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	708	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	12/08/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7818990 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	423912  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granite 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	Db1.12
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa ewartiana
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Very dark grey (10YR3/1-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.05); Clear change to - 
	A3	0.08 - 0.16 m	Dark brown (7.5YR3/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Gradual change to - 
	B1	0.16 - 0.4 m	Brown (7.5YR4/4-Moist); ; Coarse sandy light clay; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Earthy fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field
	 pH 6 (Raupach, 0.3); Gradual change to - 
	B21	0.4 - 0.7 m	Strong brown (7.5YR4/6-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common cutans, 10-
	50% of ped faces or walls coated, distinct; Common (10 - 20 %), Manganiferous, Fine (0 - 2 
	mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); Gradual 
	change to - 
	B22	0.7 - 0.9 m	Yellowish brown (10YR5/4-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common cutans, 10-
	50% of ped faces or walls coated, distinct; Common (10 - 20 %), Manganiferous, Fine (0 - 2 
	mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	708	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.7A
	0.7 - 0.9	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.7 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.7 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	708	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension