Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	713	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	12/08/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7814652 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	409902  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	10 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Grey Sodosol Thick Non-gravelly 	Principal Profile Form:	Dy3.43
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Aristida species, Bothriochloa 
	ewartiana	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Coarse sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	A2e	0.1 - 0.4 m	Light brownish grey (10YR6/2-Moist); ; Sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; 2-10%, medium gravelly, 6-20mm, subrounded, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.3); Abrupt change to - 
	B21	0.4 - 0.55 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR68, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ;
	 Medium heavy clay; Strong grade of structure, 100-200 mm, Columnar; Moderate grade of 
	structure, 50-100 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Strong 
	consistence; 2-10%, medium gravelly, 6-20mm, subrounded, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.55); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	713	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	713	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile