Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	717	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	13/08/91	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7807439 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	432779  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granite 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Rises
	3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	Dr2.12
	loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	No analytical data are available but confidence is fair.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa pertusa, Bothriochloa decipiens, 
	Heteropogon contortus	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	; Clay loam, sandy; Massive grade of structure; Earthy fabric; Dry; Very weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.2 m	; Medium heavy clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-ped 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Gradual change to - 
	B22	0.2 - 0.45 m	; Medium heavy clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-ped 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	Gradual change to - 
	C	0.45 - 1.4 m	; Sandy clay loam; Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 7.5 (Raupach, 1.4); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	717	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	717	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile