Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	720	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	13/08/91	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7801456 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	420554  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Limestone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Hills
	3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	210 degrees
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Pedal Hypercalcic Calcarosol Non-gravelly Clayey 	Principal Profile Form:	Ug5.12
	Medium Clayey Shallow
	ASC Confidence:	Great Soil Group:	Rendzina
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Very dark greyish brown (10YR3/2-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; Very few (0 - 2 %), Calcareous, 
	Fine (0 - 2 mm), Concretions; , Gypseous, , ; Soil matrix is Highly calcareous; Clear change to - 
	A/B	0.02 - 0.22 m	Very dark grey (10YR3/1-Moist); ; Light medium clay; Strong grade of structure, 2-5 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Weak consistence; 20-50%, medium gravelly, 6-20mm, 
	subrounded, dispersed, Limestone, coarse fragments; Few (2 - 10 %), Calcareous, Medium (2 -
	6 mm), Concretions; , Gypseous, , ; Soil matrix is Highly calcareous; Field pH 9.5 (Raupach, 
	0.05); Clear change to - 
	B/C	0.22 - 1.5 m	Brownish yellow (10YR6/6-Moist); ; Light clay; Massive grade of structure; Smooth-ped fabric; 
	Dry; Weak consistence; Many (20 - 50 %), Calcareous, Fine (0 - 2 mm), Veins; , Gypseous, , ; 
	Soil matrix is Highly calcareous; Field pH 9.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	720	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.22	7.9A
	0.22 - 1.5	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.22
	0.22 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.22
	0.22 - 1.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	720	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension