Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	726	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	14/08/91	Elevation:	330 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7812334 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	394953  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thin Non-gravelly Loamy 	Principal Profile Form:	Gn3.11
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 1.01-3m, Closed or dense. *Species includes - Bothriochloa ewartiana, Phynchelytrum 
	repens, Heteropogon contortus	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus papuana, Eucalyptus erythrophloia, Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, rounded, Basalt
	Profile Morphology
	A	0 - 0.08 m	Dark reddish brown (5YR3/2-Moist); ; Loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear 
	B1	0.08 - 0.4 m	Yellowish red (5YR3/6-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Earthy fabric; Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, 
	Quartz, coarse fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear change to - 
	B21	0.4 - 0.55 m	Dark red (10R3/6-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Angular blocky; 
	Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Dry; Weak consistence; 
	0-2%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.55); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	726	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	726	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile