Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	732	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	15/08/91	Elevation:	330 metres
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7807558 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	416421  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Rises
	3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Calcic Red Chromosol Thin Non-gravelly Clay-loamy 	Principal Profile Form:	Dr2.13
	Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Closed or dense. *Species includes - Bothriochloa ewartiana, Phynchelytrum 
	repens, Chrysopogon fallax	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear 
	B1	0.05 - 0.22 m	Yellowish red (5YR4/6-Moist); ; Clay loam, sandy; Weak grade of structure, 50-100 mm, 
	Angular blocky; Earthy fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Clear 
	B21	0.22 - 0.4 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Prismatic; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	B/C	0.4 - 0.65 m	Reddish brown (5YR4/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; 
	Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Soil matrix is Moderately 
	calcareous; Field pH 8.5 (Raupach, 0.6); Gradual change to - 
	C	0.65 - 1.3 m	Brown (7.5YR5/4-Moist); ; Earthy fabric; Dry; Weak consistence; Many (20 - 50 %), 
	Calcareous, Medium (2 -6 mm), Soft segregations; , Gypseous, , ; Soil matrix is Highly 
	calcareous; Field pH 9 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	732	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.6A
	0.65 - 1.3	6.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.65 - 1.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.65 - 1.3

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	732	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension