Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	30/09/91	Elevation:	290 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7730394 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	416041  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Subnatric Brown Sodosol Thick Non-gravelly 	Principal Profile Form:	Dy2.23
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa ewartiana, Chrysopogon fallax, Aristida species
	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Eucalyptus cambageana, Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus cambageana, Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy clay loam; Weak grade of structure; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.05); Clear change to - 
	A12	0.05 - 0.3 m	Brown (7.5YR4/3-Moist); ; Sandy clay loam (Light); Weak grade of structure; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9 (Raupach, 0.3); Clear change to - 
	B21	0.3 - 0.6 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Prismatic; Many (20 - 50 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 0.6); Clear change to - 
	B22k	0.6 - 0.85 m	Light yellowish brown (10YR6/4-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, 
	Prismatic; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules; Many (20 - 50 %), 
	Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.9A
	0.05 - 0.3	7.2A
	0.3 - 0.6	8.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.3
	0.3 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.3
	0.3 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	754	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension