Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	76	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	26/07/90	Elevation:	317 metres
	Map Ref.:	Sheet No. : 8056   GPS	Rainfall:	No Data
	Northing/Long.:	7730698 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	372421  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Brown Chromosol Medium Non-	Principal Profile Form:	Dy3.43
	gravelly Loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Enteropogon species, Aristida species
	Mid Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.28 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy fine sand; Massive grade of structure; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 4.8 (Raupach, 0.05); Few, fine (1-
	2mm) roots; Abrupt, Smooth change to - 
	A2e	0.28 - 0.3 m	Pale brown (10YR6/3-Moist); ; Loamy fine sand; Massive grade of structure; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.3); Few, fine (1-2mm) 
	roots; Abrupt, Smooth change to - 
	B2c	0.3 - 0.9 m	Brown (10YR5/3-Moist); Mottles, 10YR81, 20-50% , 15-30mm, Distinct; Mottles, 20-50% ; Clay 
	loam, fine sandy; Strong grade of structure, 50-100 mm, Columnar; Strong grade of structure, 
	10-20 mm, Angular blocky; Moderately moist; Very firm consistence; Many (20 - 50 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 
	6.8 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	76	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.28	5.5A	1.8B	0.71	0.37	0.05
	0.28 - 0.3	6.3A
	0.3 - 0.9	6.7A	7.1J	2.4	0.2	0.5	10.2I	4.90
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.28
	0.28 - 0.3
	0.3 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.28
	0.28 - 0.3
	0.3 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	76	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension