Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	775	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	02/10/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7721196 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	399641  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endoacidic Crusty Grey Vertosol Non-gravelly Medium fine 	Principal Profile Form:	Ug5.24
	Very fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Lysiphillum carronii, Eremophila mitchellii, Terminalia oblongata
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Acacia cambagei
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Greyish brown (10YR5/2-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Clear change to - 
	A12	0.03 - 0.3 m	Grey (10YR6/1-Moist); ; Medium clay; Massive grade of structure; Earthy fabric; Dry; Very 
	strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Gradual 
	B21	0.3 - 0.9 m	Dark grey (10YR4/1-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Common (10 - 20 %), 
	Manganiferous, Fine (0 - 2 mm), Veins; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.6); Diffuse change to - 
	B22	0.9 - 1.4 m	Light brownish grey (10YR6/2-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Very strong consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	775	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.3	6.2A
	0.3 - 0.9	6.5A
	0.9 - 1.4	5.2A	9.7J	9.4	0.1	2.2	23.9I	9.21
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.3
	0.3 - 0.9
	0.9 - 1.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.3
	0.3 - 0.9
	0.9 - 1.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	775	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension