Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	782	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	03/10/91	Elevation:	290 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7722740 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	424124  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Crusty Brown Vertosol Gravelly Medium fine 	Principal Profile Form:	Ug5.25
	Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa decipiens
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - Acacia harpophylla, Lysiphillum carronii
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, rounded, Quartzite
	Profile Morphology
	A11	0 - 0.01 m	Brown (7.5YR5/3-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, Subangular 
	blocky; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	A12	0.01 - 0.24 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, Subangular
	 blocky; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.05); Clear change to - 
	B21	0.24 - 0.5 m	Brown (7.5YR4/3-Moist); ; Medium heavy clay; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm),
	 Veins; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.3); Diffuse change to - 
	B22	0.5 - 1.9 m	Brown (7.5YR5/3-Moist); ; Medium heavy clay; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm),
	 Veins; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	782	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.24	6.7A
	0.24 - 0.5	7.5A	8.9J	9.7	0.3	3.8	23.7I	16.03
	0.5 - 1.9	6.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.24
	0.24 - 0.5
	0.5 - 1.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.24
	0.24 - 0.5
	0.5 - 1.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	782	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension