Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	799	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	15/10/91	Elevation:	230 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7699620 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	417266  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic No Available Class Stratic Rudosol Non-gravelly Loamy 	Principal Profile Form:	Uc1
	Deep  
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus polycarpa, Eucalyptus tereticornis, Eucalyptus 
	tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Loamy fine sand; Massive grade of structure; Dry; Very
	 weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to
	A12	0.05 - 0.22 m	Brown (7.5YR4/2-Moist); ; Loamy fine sand; Massive grade of structure; Dry; Firm consistence;
	 , Calcareous, , ; , Gypseous, , ; Diffuse change to - 
	C1	0.22 - 0.6 m	Brown (7.5YR5/4-Moist); ; Loamy fine sand; Massive grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); Diffuse change to - 
	C2	0.6 - 1.4 m	Brown (7.5YR5/4-Moist); ; Fine sand; Single grain grade of structure; Moderately moist; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); Diffuse change to
	C3	1.4 - 2 m	Reddish brown (5YR5/4-Moist); , 5YR73; Fine sand; Single grain grade of structure; Moderately
	 moist; Loose consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	799	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.8A
	0.22 - 0.6	6.7A
	1.4 - 2	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.22 - 0.6
	1.4 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.22 - 0.6
	1.4 - 2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	799	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension