Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	804	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	15/10/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7704218 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	397899  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Thin Non-gravelly Loamy Clay-	Principal Profile Form:	Um5.41
	loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus setosa, Planchonia careya
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus polycarpa, Eucalyptus setosa
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish grey (5YR4/2-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry;
	 Weak consistence; , Calcareous, , ; , Gypseous, , ; 
	B1	0.05 - 0.3 m	Dark reddish brown (5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; 
	B21	0.3 - 0.45 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; 
	B3	0.45 - 0.5 m	; Massive grade of structure; Dry; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Very many (50 - 100 %), Ferruginous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	804	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	804	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile