Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	807	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	16/10/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7701280 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	424284  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Black Chromosol Medium Non-gravelly Silty 	Principal Profile Form:	Dd2.42
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Sporobolus species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1j	0 - 0.01 m	Dark grey (10YR4/1-Moist); ; Silty clay loam; Massive grade of structure; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; 
	A21	0.01 - 0.12 m	Dark grey (10YR4/1-Moist); ; Silty clay loam; Massive grade of structure; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	B21	0.12 - 0.4 m	Very dark grey (10YR3/1-Moist); , 2.5Y32; Heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Strong grade of structure, 5-10 mm, Angular blocky; Dry; Very strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); 
	B22	0.4 - 1 m	Grey (10YR5/1-Moist); , 2.5Y32; Heavy clay; Moderate grade of structure, 50-100 mm, 
	Subangular blocky; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.6 
	(Raupach, 0.7); 
	B23	1 - 1.2 m	Dark grey (10YR4/1-Moist); Mottles, 2-10% , 0-5mm, Faint; Mottles, 2-10% ; Heavy clay; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Dry; Very strong consistence; , 
	Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	807	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.12	6A
	0.12 - 0.4	6.6A
	0.4 - 1	7.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.12
	0.12 - 0.4
	0.4 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.12
	0.12 - 0.4
	0.4 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	807	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension