Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	814	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	17/10/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7689044 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	422862  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Grey Sodosol Thick Non-gravelly 	Principal Profile Form:	Dy3.32
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Aristida species, Chrysopogon fallax
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, rounded, Ferricrete
	Profile Morphology
	A11	0 - 0.08 m	Black (10YR2/1-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.05); Clear change to - 
	A12	0.08 - 0.38 m	Dark greyish brown (10YR4/2-Moist); , 10YR51; Clay loam; Weak grade of structure, 10-20 mm,
	 Subangular blocky; Earthy fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 
	0.2); Clear change to - 
	A2j	0.38 - 0.4 m	; Clay loam; Earthy fabric; Dry; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B2	0.4 - 0.45 m	Dark grey (10YR4/1-Moist); , 10YR43; Heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	814	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.3A	4.9B	4.8	0.16	0.23
	0.08 - 0.38	5.4A
	0.38 - 0.4	5.5A	4.9B	6.1	0.06	0.68
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.38
	0.38 - 0.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.38
	0.38 - 0.4

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	814	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension