Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	819	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	18/10/91	Elevation:	210 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7690609 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	416936  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Grey Vertosol Non-gravelly Medium fine 	Principal Profile Form:	Ug5.24
	Very fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Dichanthium species, Iseilema vaginiflorum
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Grey (10YR5/1-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; 
	A12	0.03 - 0.38 m	Grey (10YR5/1-Moist); ; Heavy clay; Moderate grade of structure, 50-100 mm, Angular blocky; 
	Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); 
	B21	0.38 - 1 m	Dark grey (2.5Y4/1-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.7); 
	B22	1 - 1.1 m	Grey (10YR5/1-Moist); ; Heavy clay; Strong grade of structure, 10-20 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	819	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.38	7A
	1 - 1.1	6.2A	10.2J	9.4	0.1	0.8	21.1I	3.79
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.38
	1 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.38
	1 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	819	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension