Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	83	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	06/08/90	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7770624 AMG zone: 55	Runoff:	No runoff
	Easting/Lat.:	454428  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	1 % 	Aspect:	20 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol Medium Slightly gravelly 	Principal Profile Form:	Uc5.11
	Sandy Sandy Deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Aristida species, Eragrostis species
	Mid Strata - Shrub, 3.01-6m, Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.22 m	Reddish brown (5YR4/4-Moist); ; Coarse sand; Single grain grade of structure; Earthy fabric; 
	Dry; Loose consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.05); Abundant, 
	medium (2-5mm) roots; Clear, Smooth change to - 
	B21	0.22 - 0.7 m	Red (2.5YR4/8-Moist); ; Coarse sand; Single grain grade of structure; Earthy fabric; Dry; Loose 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 8.8 (Raupach, 0.3); Common, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	B22	0.7 - 1.05 m	Red (2.5YR4/8-Moist); ; Clayey coarse sand; Single grain grade of structure; Earthy fabric; Dry;
	 Loose consistence; 10-20%, medium gravelly, 6-20mm, angular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	83	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.22	7.9A	4.4B	0.23	0.07	0.03
	0.22 - 0.7	8.3A	2.2J	0.5	0.1	0.2	1.7I	11.76
	0.7 - 1.05	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.22
	0.22 - 0.7
	0.7 - 1.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.22
	0.22 - 0.7
	0.7 - 1.05

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	83	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension